A close up of a sign

Description automatically generated

**Weekly Eyewash Testing Log**

**Version 1. 02/16/2024**

# GENERAL REQUIREMENTS:

The emergency eyewash station must be checked weekly for the following:

* Accessibility of the eyewash station is clear of any obstructions
* Eyewash fixture is in good condition and is free of any leaks
* Nozzle dust covers/caps are in place and are operating properly
* Flush water for at least 2 minutes or until clear water flows continuously

# LOCATION:

Principal Investigator / Area Supervisor:

Room Number:

Initial upon completion of weekly testing.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Year** | **Week 1** | **Week 2** | **Week 3** | **Week 4** | **Week 5** | **Comments** |
| **January** |  |  |  |  |  |  |
| **February** |  |  |  |  |  |  |
| **March** |  |  |  |  |  |  |
| **April** |  |  |  |  |  |  |
| **May** |  |  |  |  |  |  |
| **June** |  |  |  |  |  |  |
| **July** |  |  |  |  |  |  |
| **August** |  |  |  |  |  |  |
| **September** |  |  |  |  |  |  |
| **October** |  |  |  |  |  |  |
| **November** |  |  |  |  |  |  |
| **December** |  |  |  |  |  |  |